---
id: TASK-3
title: 3D print prototype frame — stealth integrated design
status: To Do
assignee: []
created_date: '2026-02-22 00:44'
labels: []
dependencies: []
priority: medium
---

## Description

<!-- SECTION:DESCRIPTION:BEGIN -->
Print the integrated frame from integrated_frame.scad in PETG matte black. Verify LED channel dimensions, filter slot fit, temple wire routing, battery cavity, and hinge mechanism. Test-fit IR filter strip (cut from Wratten 87C gel sheet). Adjust parametric dimensions as needed.
<!-- SECTION:DESCRIPTION:END -->

## Acceptance Criteria
<!-- AC:BEGIN -->
- [ ] #1 Frame printed in PETG, no warping
- [ ] #2 IR filter strip press-fits into brow bar slot
- [ ] #3 Flex PCB strip slides into channel cleanly
- [ ] #4 Battery fits in temple tip cavity
- [ ] #5 Charge port accessible from underside
<!-- AC:END -->
